(kicad_pcb
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting
			(front yes)
			(back yes)
		)
		(covering
			(front no)
			(back no)
		)
		(plugging
			(front no)
			(back no)
		)
		(capping no)
		(filling no)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12)
			(dashed_line_gap_ratio 3)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(footprint "Package_DIP:DIP-4_W7.62mm"
		(layer "B.Cu")
		(uuid "3f524982-43a1-4498-834b-5ed3050ef103")
		(at 114.3 99.06)
		(descr "4-lead though-hole mounted DIP package, row spacing 7.62mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U1"
			(at 3.81 2.33 180)
			(layer "B.SilkS")
			(uuid "127ec338-c515-49e8-b931-7a6c1bcd14d5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "PC817"
			(at 3.81 -4.87 180)
			(layer "B.Fab")
			(uuid "0986a0c3-e565-4ea5-8ef2-ebf96f608b72")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" "http://www.soselectronic.cz/a_info/resource/d/pc817.pdf"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "8fd086f4-7c23-4fba-9ce9-37e74ad7198a")
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify mirror)
			)
		)
		(property "Description" "DC Optocoupler, Vce 35V, CTR 50-300%, DIP-4"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "93a85276-a50d-4a4b-9830-891228697992")
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify mirror)
			)
		)
		(property "KiLib_Generator" "package/DIP/legacy"
			(at 0 0 180)
			(layer "B.SilkS")
			(hide yes)
			(uuid "219e8bad-ea29-497f-80b4-92e5e872c395")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm*")
		(path "/d8d449b5-9d9f-42e3-8a8b-35de2680c75d")
		(sheetname "/")
		(sheetfile "PCB.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2" "4" "3")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start 1.16 -3.87)
			(end 6.46 -3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "5d0c2059-a501-42e7-bbdd-6ef6d60540ed")
		)
		(fp_line
			(start 1.16 1.33)
			(end 1.16 -3.87)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "87c7c8fe-e6b1-48ec-b52b-b1a8b5a132b2")
		)
		(fp_line
			(start 2.81 1.33)
			(end 1.16 1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "cb3cb0af-687a-4ca7-a74c-e34418ed731d")
		)
		(fp_line
			(start 6.46 -3.87)
			(end 6.46 1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "e8fc5b14-56b9-4ca5-b6db-3dbfe9b19413")
		)
		(fp_line
			(start 6.46 1.33)
			(end 4.81 1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "85b1c5f6-fe0d-45b3-8d49-5757d960e56c")
		)
		(fp_arc
			(start 2.81 1.33)
			(mid 3.81 0.33)
			(end 4.81 1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "3496615f-21ea-40a8-81e9-41751a7a30d1")
		)
		(fp_rect
			(start -1.06 1.52)
			(end 8.67 -4.07)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "B.CrtYd")
			(uuid "8e6d039f-672e-4868-82cc-3dce52c2e8eb")
		)
		(fp_line
			(start 0.635 -3.81)
			(end 0.635 0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "5fba3706-9486-4092-8ae5-28ec031a49b6")
		)
		(fp_line
			(start 0.635 0.27)
			(end 1.635 1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "88ce8a6c-e8be-4a2e-b293-b3eb42812503")
		)
		(fp_line
			(start 1.635 1.27)
			(end 6.985 1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "34443282-24ad-46ef-93b3-2ee6baf2d685")
		)
		(fp_line
			(start 6.985 -3.81)
			(end 0.635 -3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "0ee7dd35-fc87-4b38-8601-0e287e494058")
		)
		(fp_line
			(start 6.985 1.27)
			(end 6.985 -3.81)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "55ad56c7-2270-4125-b266-71959db72e96")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 -1.27 180)
			(layer "B.Fab")
			(uuid "46d654f4-1983-4643-b30c-5c37374d44bc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(point
			(at 118.11 97.79)
			(size 1.27)
			(layer "B.Fab")
			(uuid "d5e93b68-da30-40c2-9193-1ae09acfff63")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net "Net-(R2-Pad2)")
			(pintype "passive")
			(uuid "f59f1680-20df-4431-a5f6-4553521381b3")
		)
		(pad "2" thru_hole circle
			(at 0 -2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J1-GND-Pad14)")
			(pintype "passive")
			(uuid "cb7242e5-8253-40f1-ab3d-6a236cc83c23")
		)
		(pad "3" thru_hole circle
			(at 7.62 -2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J2-Pin_2)")
			(pintype "passive")
			(uuid "6af0cedb-80b2-4c63-b30a-dfe5e362f7e9")
		)
		(pad "4" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J2-Pin_1)")
			(pintype "passive")
			(uuid "df670244-d9e5-4ef5-a1f9-1cc4c6d4b39c")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-4_W7.62mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "B.Cu")
		(uuid "4c770bf3-c8d1-4b97-a2d0-6fa7e6d5c2e8")
		(at 104.14 99.06)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R2"
			(at 3.81 2.37 180)
			(layer "B.SilkS")
			(uuid "7dbc3899-afed-4ea8-adb2-ceafa96562fc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "200"
			(at 3.81 -2.37 180)
			(layer "B.Fab")
			(uuid "1cc68101-30a8-4291-ac86-25620beec2ca")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "df62af97-0511-4892-beff-7d80fbc5e6d6")
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify mirror)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
			(uuid "53f41757-5754-4e04-ab59-7834df32684b")
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify mirror)
			)
		)
		(property "KiLib_Generator" "resistor/THT"
			(at 0 0 180)
			(layer "B.SilkS")
			(hide yes)
			(uuid "149759a5-543e-463f-8519-256907676cfa")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/789a62b9-e75c-47fa-84f6-c89be29171da")
		(sheetname "/")
		(sheetfile "PCB.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start 0.54 -1.37)
			(end 7.08 -1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "9df1df1f-e36e-49ba-b77f-25bd551be0c9")
		)
		(fp_line
			(start 0.54 -1.04)
			(end 0.54 -1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "a5669392-4b82-4805-b819-848d3331d1a4")
		)
		(fp_line
			(start 0.54 1.04)
			(end 0.54 1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "38d2e1a6-b7b0-4bd7-98ef-7c629eee9ce6")
		)
		(fp_line
			(start 0.54 1.37)
			(end 7.08 1.37)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "6b6bb4c9-5436-4e54-941a-6b8e86411451")
		)
		(fp_line
			(start 7.08 -1.37)
			(end 7.08 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "2043ca9f-478f-430e-9a1d-0b22426e24e3")
		)
		(fp_line
			(start 7.08 1.37)
			(end 7.08 1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "15623721-3b7a-44f3-b9ce-feb3125f09a2")
		)
		(fp_rect
			(start -1.05 1.5)
			(end 8.67 -1.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "B.CrtYd")
			(uuid "14b21cfe-ea7c-4ed2-8250-c2f22176f95e")
		)
		(fp_line
			(start 0 0)
			(end 0.66 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "fad498eb-a568-43ac-8167-af88e5fda962")
		)
		(fp_line
			(start 7.62 0)
			(end 6.96 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "3249456e-4d3d-4091-a42c-b51d48ed47bd")
		)
		(fp_rect
			(start 0.66 1.25)
			(end 6.96 -1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "B.Fab")
			(uuid "a8ff59ec-9cf2-4614-8529-668abe84e6c8")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 180)
			(layer "B.Fab")
			(uuid "e2637980-855c-4de7-b0e2-b55bf72baccf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J1-GPIO24{slash}SDIO_DAT0)")
			(pintype "passive")
			(uuid "b95d22f8-b9cc-475d-9166-12817b0ac2b0")
		)
		(pad "2" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(R2-Pad2)")
			(pintype "passive")
			(uuid "a4e4baa0-58c1-4763-821b-40e340e78d77")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical"
		(layer "B.Cu")
		(uuid "cfe81f41-2dec-43dd-85bd-dd837a9633b5")
		(at 129.54 99.06 90)
		(descr "JST XH series connector, B2B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf)")
		(tags "connector JST XH vertical")
		(property "Reference" "J2"
			(at 1.25 3.55 90)
			(layer "B.SilkS")
			(uuid "5ce25497-4bfe-46e2-bda4-21e006c27414")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "Conn_01x02"
			(at 1.25 -4.6 90)
			(layer "B.Fab")
			(uuid "68e125c0-1ff4-43a6-983b-b376c7d40661")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
			(uuid "21799d9d-5f1e-4281-bcae-a8b562c14152")
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify mirror)
			)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
			(uuid "bf92ded1-5ba3-49d6-9840-01022daf1af9")
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify mirror)
			)
		)
		(property "KiLib_Generator" "connector/JST"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
			(uuid "925cb775-8d8f-4cc9-84e6-23bd6f1fd6ad")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/ab8966d1-405b-408e-8002-0e78ecac2794")
		(sheetname "/")
		(sheetfile "PCB.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start 4.3 -2.75)
			(end 1.25 -2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "079087d5-b137-4fa4-b9cd-eeaaee78f3ea")
		)
		(fp_line
			(start -1.8 -2.75)
			(end 1.25 -2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "5b7edf0c-c05e-49f6-a4b7-c2955eb3b004")
		)
		(fp_line
			(start 5.05 0.2)
			(end 4.3 0.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "b0c4d381-ac59-452f-9d6e-c3afe4504956")
		)
		(fp_line
			(start 4.3 0.2)
			(end 4.3 -2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "841fb94d-9a06-4b3a-93d1-3b0e676a7266")
		)
		(fp_line
			(start -1.8 0.2)
			(end -1.8 -2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "92f27c7b-025f-4f0c-844d-d8fdafe9ba9b")
		)
		(fp_line
			(start -2.55 0.2)
			(end -1.8 0.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "2a48bc34-f4a1-4b1d-a772-25d3b394078f")
		)
		(fp_line
			(start -1.6 2.75)
			(end -2.85 2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "cefb2ddb-9ca8-4f31-8049-1a32c58cca2f")
		)
		(fp_line
			(start -2.85 2.75)
			(end -2.85 1.5)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "ff3f0dc5-362d-4f88-9738-e8dfee9a5c9f")
		)
		(fp_rect
			(start 3.25 2.45)
			(end 5.05 1.7)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "B.SilkS")
			(uuid "8b355592-e8b3-4364-b595-de26f926e564")
		)
		(fp_rect
			(start 0.75 2.45)
			(end 1.75 1.7)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "B.SilkS")
			(uuid "5306a102-2614-4c0d-a124-935bf1e8f86a")
		)
		(fp_rect
			(start -2.55 2.45)
			(end -0.75 1.7)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "B.SilkS")
			(uuid "b2bfdb2e-d712-4502-8d03-c30a73a5856c")
		)
		(fp_rect
			(start -2.56 2.46)
			(end 5.06 -3.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "B.SilkS")
			(uuid "2ebc6d8c-376f-4946-899f-c9c1ac8052c7")
		)
		(fp_rect
			(start -2.95 2.85)
			(end 5.45 -3.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "B.CrtYd")
			(uuid "6b44591b-240e-4a3a-8291-37973cdea800")
		)
		(fp_line
			(start 0 1.35)
			(end 0.625 2.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "7e2ff888-20a0-45c6-a233-bafdc4973ce0")
		)
		(fp_line
			(start -0.625 2.35)
			(end 0 1.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "17718847-f2c7-4fab-898f-5c2b354ee490")
		)
		(fp_rect
			(start -2.45 2.35)
			(end 4.95 -3.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "B.Fab")
			(uuid "6cb47c15-b2a8-46d7-aa0e-85e7159477ad")
		)
		(fp_text user "${REFERENCE}"
			(at 1.25 -2.7 90)
			(layer "B.Fab")
			(uuid "939e0403-041d-493c-89f5-b23818997671")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net "Net-(J2-Pin_1)")
			(pinfunction "Pin_1_1")
			(pintype "passive")
			(uuid "2f2f50ef-f4f8-4317-b9bf-1c5bcd14892a")
		)
		(pad "2" thru_hole oval
			(at 2.5 0 90)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J2-Pin_2)")
			(pinfunction "Pin_2_2")
			(pintype "passive")
			(uuid "a4e1089a-6ad6-4462-abdf-d165c39462a5")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_2x20_P2.54mm_Vertical"
		(layer "B.Cu")
		(uuid "d1964e02-fdd4-481a-b18d-2c10909f6989")
		(at 99.06 78.74 180)
		(descr "Through hole straight socket strip, 2x20, 2.54mm pitch, double rows (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 2x20 2.54mm double row")
		(property "Reference" "J1"
			(at -1.27 2.77 0)
			(layer "B.SilkS")
			(uuid "0747ace3-9c9e-484e-b3ad-12c20652b5df")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Value" "Raspberry_Pi_4"
			(at -1.27 -51.03 0)
			(layer "B.Fab")
			(uuid "0a9fe9e5-c9bc-40e8-9c36-9107ee4e579a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property "Datasheet" "https://datasheets.raspberrypi.com/rpi4/raspberry-pi-4-datasheet.pdf"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
			(uuid "6b7c594e-852f-461d-ac03-520806377459")
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify mirror)
			)
		)
		(property "Description" "Raspberry Pi 4 Model B"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
			(uuid "d2f1d437-6f17-49f3-a6bf-730528084ddd")
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify mirror)
			)
		)
		(property "KiLib_Generator" "connector/pin_header_socket"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
			(uuid "d5ffc61f-9a20-490b-ab04-288c8958bb6b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(property ki_fp_filters "PinHeader*2x20*P2.54mm*Vertical* PinSocket*2x20*P2.54mm*Vertical*")
		(path "/bf0cbcc3-30b6-4a44-9549-fee0375b9972")
		(sheetname "/")
		(sheetfile "PCB.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "32" "33" "8" "10" "36" "11" "12" "35" "38" "40" "15" "16" "18"
					"22" "37" "13" "30" "6" "25" "9" "14" "20" "34" "39" "2" "4" "1" "17"
					"27" "28" "3" "5" "7" "29" "31" "26" "24" "21" "19" "23"
				)
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start 1.33 1.33)
			(end 1.33 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "379c7d79-f830-4825-b312-c3d8e03f9967")
		)
		(fp_line
			(start 1.33 -1.27)
			(end 1.33 -49.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "20704ba9-284f-499f-bf4b-6644f8a0ef7d")
		)
		(fp_line
			(start 0 1.33)
			(end 1.33 1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "a9b28315-4faf-4ae0-8e02-e0d420cb0eed")
		)
		(fp_line
			(start -1.27 1.33)
			(end -1.27 -1.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "489b9d95-9894-4427-a76c-5ecf3a462f67")
		)
		(fp_line
			(start -1.27 -1.27)
			(end 1.33 -1.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "0e9a0ad4-a124-40de-8edb-0a462c49423f")
		)
		(fp_line
			(start -3.87 1.33)
			(end -1.27 1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "f91bf419-9bd1-49af-91bd-a4ba35dbe7b7")
		)
		(fp_line
			(start -3.87 1.33)
			(end -3.87 -49.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "91d4fdd2-b6f1-48f4-9ce2-45c0ece29a46")
		)
		(fp_line
			(start -3.87 -49.59)
			(end 1.33 -49.59)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "B.SilkS")
			(uuid "684eb1bd-b1a0-4e0a-aa1f-43369671bc09")
		)
		(fp_line
			(start 1.77 1.77)
			(end 1.77 -50.03)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "ad932d86-e9a0-48f0-bd2a-1989baf30c1d")
		)
		(fp_line
			(start 1.77 -50.03)
			(end -4.31 -50.03)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "22865b96-9408-44fe-8a5f-3e6be9f6425e")
		)
		(fp_line
			(start -4.31 1.77)
			(end 1.77 1.77)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "e0a277ee-f9f1-44e6-8d4f-0758656a5ea1")
		)
		(fp_line
			(start -4.31 -50.03)
			(end -4.31 1.77)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "B.CrtYd")
			(uuid "19fcb1b5-7506-4a41-8af2-11292d5dc70d")
		)
		(fp_line
			(start 1.27 0.27)
			(end 1.27 -49.53)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "f9e8d4d4-aaaa-4dab-8175-e807a912f537")
		)
		(fp_line
			(start 1.27 -49.53)
			(end -3.81 -49.53)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "a0ba7099-92f8-4b4c-9756-cad3b12a106c")
		)
		(fp_line
			(start 0.27 1.27)
			(end 1.27 0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "bdddfac2-6234-48bf-821f-af268c6606eb")
		)
		(fp_line
			(start -3.81 1.27)
			(end 0.27 1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "42222e3c-ac2a-4175-8457-d2976d087216")
		)
		(fp_line
			(start -3.81 -49.53)
			(end -3.81 1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "B.Fab")
			(uuid "a40f2c5f-54fa-494c-86bf-7df5fbdf9943")
		)
		(fp_text user "${REFERENCE}"
			(at -1.27 -24.13 90)
			(layer "B.Fab")
			(uuid "c160a7e7-5722-4407-a9dd-bd96eeb7f204")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify mirror)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J1-3V3-Pad1)")
			(pinfunction "3V3_1")
			(pintype "power_out")
			(uuid "e6c7b816-3d4c-42f2-aed2-edb645582b48")
		)
		(pad "2" thru_hole circle
			(at -2.54 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J1-5V-Pad2)")
			(pinfunction "5V_2")
			(pintype "power_out")
			(uuid "fa007ff5-94d9-472d-aa3e-59a8f62c9de5")
		)
		(pad "3" thru_hole circle
			(at 0 -2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J1-SDA_I2C1{slash}GPIO02-Pad3)")
			(pinfunction "SDA_I2C1/GPIO02_3")
			(pintype "bidirectional")
			(uuid "5995742a-ecef-4897-9f8f-673b575fe607")
		)
		(pad "4" thru_hole circle
			(at -2.54 -2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J1-5V-Pad2)")
			(pinfunction "5V_4")
			(pintype "passive")
			(uuid "62747139-1595-45d4-9ad9-defd2f0acba3")
		)
		(pad "5" thru_hole circle
			(at 0 -5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J1-SCL_I2C1{slash}GPIO03-Pad5)")
			(pinfunction "SCL_I2C1/GPIO03_5")
			(pintype "bidirectional")
			(uuid "41c0fb14-043a-435e-9e86-b02000ae0a56")
		)
		(pad "6" thru_hole circle
			(at -2.54 -5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J1-GND-Pad14)")
			(pinfunction "GND_6")
			(pintype "power_out")
			(uuid "a8330200-e2c7-4ff4-bead-2034658a1011")
		)
		(pad "7" thru_hole circle
			(at 0 -7.62 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J1-GPCLK0{slash}GPIO04-Pad7)")
			(pinfunction "GPCLK0/GPIO04_7")
			(pintype "bidirectional")
			(uuid "fcf10185-a479-4d0f-9828-af7846b93a80")
		)
		(pad "8" thru_hole circle
			(at -2.54 -7.62 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J1-GPIO14{slash}UART_TXD-Pad8)")
			(pinfunction "GPIO14/UART_TXD_8")
			(pintype "bidirectional")
			(uuid "42c0e2c5-1ee7-4272-99ae-a0a738484c37")
		)
		(pad "9" thru_hole circle
			(at 0 -10.16 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J1-GND-Pad14)")
			(pinfunction "GND_9")
			(pintype "passive")
			(uuid "a5e67932-b93a-4ee7-8932-af866daa331d")
		)
		(pad "10" thru_hole circle
			(at -2.54 -10.16 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J1-GPIO15{slash}UART_RXD-Pad10)")
			(pinfunction "GPIO15/UART_RXD_10")
			(pintype "bidirectional")
			(uuid "af345854-7954-4b1a-b651-580627f6c038")
		)
		(pad "11" thru_hole circle
			(at 0 -12.7 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J1-GPIO17{slash}SPI1_~{CE1}-Pad11)")
			(pinfunction "GPIO17/SPI1_~{CE1}_11")
			(pintype "bidirectional")
			(uuid "a2967cf5-61af-49f2-80f9-3082d511709d")
		)
		(pad "12" thru_hole circle
			(at -2.54 -12.7 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J1-GPIO18{slash}SPI1_~{CE0}{slash}PCM_CLK{slash}PWM0-Pad12)")
			(pinfunction "GPIO18/SPI1_~{CE0}/PCM_CLK/PWM0_12")
			(pintype "bidirectional")
			(uuid "dd8264a8-0f97-4a5a-b547-4bab93966009")
		)
		(pad "13" thru_hole circle
			(at 0 -15.24 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J1-GPIO27{slash}SDIO_DAT3-Pad13)")
			(pinfunction "GPIO27/SDIO_DAT3_13")
			(pintype "bidirectional")
			(uuid "68409829-6f13-4b5a-b4df-4288956b8b11")
		)
		(pad "14" thru_hole circle
			(at -2.54 -15.24 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J1-GND-Pad14)")
			(pinfunction "GND_14")
			(pintype "passive")
			(uuid "e46605cf-74fc-4019-b000-b883857c5653")
		)
		(pad "15" thru_hole circle
			(at 0 -17.78 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J1-GPIO22{slash}SDIO_CLK-Pad15)")
			(pinfunction "GPIO22/SDIO_CLK_15")
			(pintype "bidirectional")
			(uuid "6ab78d4a-278b-42a4-b197-6dc08d80fecd")
		)
		(pad "16" thru_hole circle
			(at -2.54 -17.78 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J1-GPIO23{slash}SDIO_CMD-Pad16)")
			(pinfunction "GPIO23/SDIO_CMD_16")
			(pintype "bidirectional")
			(uuid "9b75c3af-2441-46a8-973b-befeaf2a35c9")
		)
		(pad "17" thru_hole circle
			(at 0 -20.32 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J1-3V3-Pad1)")
			(pinfunction "3V3_17")
			(pintype "passive")
			(uuid "2bf14718-3a84-4b33-ab62-9d0c7cfd1ab9")
		)
		(pad "18" thru_hole circle
			(at -2.54 -20.32 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J1-GPIO24{slash}SDIO_DAT0)")
			(pinfunction "GPIO24/SDIO_DAT0_18")
			(pintype "bidirectional")
			(uuid "645bcaa5-ff31-4f1c-85d6-be01b3f418ab")
		)
		(pad "19" thru_hole circle
			(at 0 -22.86 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J1-MOSI_SPI0{slash}GPIO10-Pad19)")
			(pinfunction "MOSI_SPI0/GPIO10_19")
			(pintype "bidirectional")
			(uuid "87474b7f-36ad-470d-a5ba-3c4893ba8023")
		)
		(pad "20" thru_hole circle
			(at -2.54 -22.86 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J1-GND-Pad14)")
			(pinfunction "GND_20")
			(pintype "passive")
			(uuid "010bf326-f3bd-450a-95d7-4e9eb0657031")
		)
		(pad "21" thru_hole circle
			(at 0 -25.4 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J1-MISO_SPI0{slash}GPIO09-Pad21)")
			(pinfunction "MISO_SPI0/GPIO09_21")
			(pintype "bidirectional")
			(uuid "9eb87101-a06f-4432-9fc1-9c46bfdb3cd7")
		)
		(pad "22" thru_hole circle
			(at -2.54 -25.4 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J1-GPIO25{slash}SDIO_DAT1-Pad22)")
			(pinfunction "GPIO25/SDIO_DAT1_22")
			(pintype "bidirectional")
			(uuid "f7fb9357-bc9c-432d-9716-611907e1a00c")
		)
		(pad "23" thru_hole circle
			(at 0 -27.94 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J1-SCLK_SPI0{slash}GPIO11-Pad23)")
			(pinfunction "SCLK_SPI0/GPIO11_23")
			(pintype "bidirectional")
			(uuid "4a3f2891-5185-4aa3-8874-4c015dd5b5c2")
		)
		(pad "24" thru_hole circle
			(at -2.54 -27.94 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J1-~{CE0}_SPI0{slash}GPIO08-Pad24)")
			(pinfunction "~{CE0}_SPI0/GPIO08_24")
			(pintype "bidirectional")
			(uuid "d4e017f8-7d02-48cf-b0db-2e4ff32f014c")
		)
		(pad "25" thru_hole circle
			(at 0 -30.48 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J1-GND-Pad14)")
			(pinfunction "GND_25")
			(pintype "passive")
			(uuid "5c9ee8eb-33e6-47fe-9dbc-4ffc7c2e1ca8")
		)
		(pad "26" thru_hole circle
			(at -2.54 -30.48 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J1-~{CE1}_SPI0{slash}GPIO07-Pad26)")
			(pinfunction "~{CE1}_SPI0/GPIO07_26")
			(pintype "bidirectional")
			(uuid "0223dbaa-e942-472e-9e5f-e02be9896b5a")
		)
		(pad "27" thru_hole circle
			(at 0 -33.02 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J1-ID_SD_I2C0{slash}GPIO00-Pad27)")
			(pinfunction "ID_SD_I2C0/GPIO00_27")
			(pintype "bidirectional")
			(uuid "f7834d96-ee65-49b2-8d4d-86a4d3f21873")
		)
		(pad "28" thru_hole circle
			(at -2.54 -33.02 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J1-ID_SC_I2C0{slash}GPIO01-Pad28)")
			(pinfunction "ID_SC_I2C0/GPIO01_28")
			(pintype "bidirectional")
			(uuid "20ff3cfe-4e04-4a55-8b91-3a445873fb2a")
		)
		(pad "29" thru_hole circle
			(at 0 -35.56 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J1-GPCLK1{slash}GPIO05-Pad29)")
			(pinfunction "GPCLK1/GPIO05_29")
			(pintype "bidirectional")
			(uuid "b6721af5-81d8-4748-bfd8-412df640b684")
		)
		(pad "30" thru_hole circle
			(at -2.54 -35.56 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J1-GND-Pad14)")
			(pinfunction "GND_30")
			(pintype "passive")
			(uuid "0f44e00a-8840-4aef-a68a-9c41f4a558ba")
		)
		(pad "31" thru_hole circle
			(at 0 -38.1 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J1-GPCLK2{slash}GPIO06-Pad31)")
			(pinfunction "GPCLK2/GPIO06_31")
			(pintype "bidirectional")
			(uuid "8e742be3-1a08-4680-8e9a-345369022a00")
		)
		(pad "32" thru_hole circle
			(at -2.54 -38.1 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J1-GPIO12{slash}PWM0-Pad32)")
			(pinfunction "GPIO12/PWM0_32")
			(pintype "bidirectional")
			(uuid "b23c3917-b6db-4538-9a65-0f3a708b1629")
		)
		(pad "33" thru_hole circle
			(at 0 -40.64 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J1-GPIO13{slash}PWM1-Pad33)")
			(pinfunction "GPIO13/PWM1_33")
			(pintype "bidirectional")
			(uuid "ecb14b3a-f760-49dd-bcff-4ac80777a5e8")
		)
		(pad "34" thru_hole circle
			(at -2.54 -40.64 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J1-GND-Pad14)")
			(pinfunction "GND_34")
			(pintype "passive")
			(uuid "dc3ccc7d-dc74-458d-b5e4-798674264647")
		)
		(pad "35" thru_hole circle
			(at 0 -43.18 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J1-GPIO19{slash}SPI1_MISO{slash}PCM_FS-Pad35)")
			(pinfunction "GPIO19/SPI1_MISO/PCM_FS_35")
			(pintype "bidirectional")
			(uuid "ec8065b6-0fc3-482f-9f65-07f0639cca43")
		)
		(pad "36" thru_hole circle
			(at -2.54 -43.18 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J1-GPIO16{slash}SPI1_~{CE2}-Pad36)")
			(pinfunction "GPIO16/SPI1_~{CE2}_36")
			(pintype "bidirectional")
			(uuid "8ddc2686-f8bc-4d13-b7b2-9219a3b6e979")
		)
		(pad "37" thru_hole circle
			(at 0 -45.72 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J1-GPIO26{slash}SDIO_DAT2-Pad37)")
			(pinfunction "GPIO26/SDIO_DAT2_37")
			(pintype "bidirectional")
			(uuid "53199164-f05b-435d-b311-779d7be0b696")
		)
		(pad "38" thru_hole circle
			(at -2.54 -45.72 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J1-GPIO20{slash}SPI1_MOSI{slash}PCM_DIN{slash}PWM1-Pad38)")
			(pinfunction "GPIO20/SPI1_MOSI/PCM_DIN/PWM1_38")
			(pintype "bidirectional")
			(uuid "e9302e42-b955-47b1-b2e9-28e1bbebb6fe")
		)
		(pad "39" thru_hole circle
			(at 0 -48.26 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J1-GND-Pad14)")
			(pinfunction "GND_39")
			(pintype "passive")
			(uuid "515a5f1a-6a49-4b6a-89cb-c5ad00f87f7b")
		)
		(pad "40" thru_hole circle
			(at -2.54 -48.26 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J1-GPIO21{slash}SPI1_SCLK{slash}PCM_DOUT-Pad40)")
			(pinfunction "GPIO21/SPI1_SCLK/PCM_DOUT_40")
			(pintype "bidirectional")
			(uuid "8ee56370-bd9e-400d-b7c1-89aa53bb3c41")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x20_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 93.98 73.66)
		(end 134.62 73.66)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "9235e32f-afb2-460c-99fd-d4801e72ebe2")
	)
	(gr_line
		(start 93.98 132.08)
		(end 93.98 73.66)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "54685c5d-5c22-4249-abf7-2576977e3d38")
	)
	(gr_line
		(start 134.62 73.66)
		(end 134.62 132.08)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "8c90a270-44a3-42e0-89a4-4b454480b40f")
	)
	(gr_line
		(start 134.62 132.08)
		(end 93.98 132.08)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "3011760e-706e-4390-a604-e1e1b9b76063")
	)
	(segment
		(start 111.76 99.06)
		(end 114.3 99.06)
		(width 1)
		(layer "F.Cu")
		(net "Net-(R2-Pad2)")
		(uuid "3df7e232-b55c-46a3-ac99-11073c0c31a2")
	)
	(segment
		(start 101.6 101.6)
		(end 104.14 101.6)
		(width 1)
		(layer "F.Cu")
		(net "Net-(J1-GND-Pad14)")
		(uuid "135d3981-a218-4848-a1a5-0ee7c0b80f29")
	)
	(segment
		(start 109.22 96.52)
		(end 114.3 96.52)
		(width 1)
		(layer "F.Cu")
		(net "Net-(J1-GND-Pad14)")
		(uuid "df4ea486-8953-4269-bb8f-d5fb17562e58")
	)
	(segment
		(start 104.14 101.6)
		(end 109.22 96.52)
		(width 1)
		(layer "F.Cu")
		(net "Net-(J1-GND-Pad14)")
		(uuid "f31ee8ef-5a0c-4f8a-a3df-66cc97e52b80")
	)
	(segment
		(start 121.92 96.52)
		(end 129.5 96.52)
		(width 1)
		(layer "F.Cu")
		(net "Net-(J2-Pin_2)")
		(uuid "bc265c3e-680b-4fc3-a805-9ef3e67b10c8")
	)
	(segment
		(start 129.5 96.52)
		(end 129.54 96.56)
		(width 1)
		(layer "F.Cu")
		(net "Net-(J2-Pin_2)")
		(uuid "c0306922-ad96-4368-b0c8-041ecde29fd6")
	)
	(segment
		(start 121.92 99.06)
		(end 129.54 99.06)
		(width 1)
		(layer "F.Cu")
		(net "Net-(J2-Pin_1)")
		(uuid "2176ef2f-2ba5-4d6d-a292-913a4a46bb2d")
	)
	(segment
		(start 101.6 99.06)
		(end 104.14 99.06)
		(width 1)
		(layer "F.Cu")
		(net "Net-(J1-GPIO24{slash}SDIO_DAT0)")
		(uuid "e9311985-2dce-4abe-985f-63a3d15b8296")
	)
	(embedded_fonts no)
)
